**BPQ Mail and Chat Server BBS User and SYSOP commands.**

? or Help:

 Displays a list of commands.

A :

 Abort the BBS output while paging.

B or Bye :

 Disconnects from the BBS.

Home :

 Enters or modifies the Home BBS. A point deletes the current Home BBS.

I :

 Display sysop - provided information about this BBS.

I callsign :

 Gives the information on callsign taken from the white pages database.

 Callsign can include wildcards.

I@ bbs :

 Gives the users of BBS found in the WP database.

IH route :

 Gives the users of the hierarchical route area from the WP database.

IZ Zip :

 Gives the users of the ZIP code area from WP database.

**K-commands delete messages sent by you or to you.**

K msg# : Deletes a message identified by its number.

KM : Deletes all the messages addressed to you, that you haven't yet read.

**L-commands list message headers.**

L : Lists the new messages since the last usage of this command.

Lx : List messages with status "x" - x can be D F N Y $.

LB : Lists bulletins.

LC : Lists all Bulletin "categories" (TO Fields)

LM : Lists the messages to you.

LL n: Lists the last n messages.

LR : Equivalent to L but the messages are listed in reverse order.

LT : List Traffic (NTS-messages).

L< Callsign : Lists message from [Callsign].

L> Callsign : Lists messages to [Callsign].

L@ [BBS] : Lists the messages VIA BBS.

L msg#- : Lists all messages, starting from msg#

L msg#-msg# : Lists messages between the given numbers.

N :

 Enters or modifies the name (max 12 characters allowed).

OP nbr of lines :

 Enables or disables the paging of output.

POLLRMS :

 Enables or disables polling RMS for messages for you.

 POLLRMS Enable

 POLLRMS Disable

 POLLRMS SSID1 SSID2 SSID2 (for the base call, specify SSID of 0)

 eg POLLRMS 0 1 15 will look for messages to CALL, CALL-1, CALL-15

 The sysop can also set the flags for other users.

 eg POLLRMS G8BPQ Enable

Q :

 Enters or modifies QTH.

**R-commands read messages.**

R msg# msg# : Reads the messages by their numbers.

RM : Reads new messages to you.

**S-commands send messages.**

S[type] callsign : Sends a message or a bulletin.

 If the type is not specified, it will be sent as private.

SP callsign : Sends a private message.

S callsign @ BBSCALLSIGN : Sends a message to a station AT another BBS.

 The message must be terminated by a Ctrl/Z or /EX followed by a return.

SC Msg# Callsign @ BBSCALLSIGN : Copies a message or bulletin to the specified callsign.

SR Msg# : Replies to a message.

V :

 Displays Version number of the BBS and Node software.

Z :

 Enters or modifies the Zip Code.

**The following commands can only be used by the SYSOP**

AUTH : Authenticate for Remote SYSOP access. Use program BPQAUTH to generate passcode..

EXPORT : Export Message to a file. Type EXPORT for details.

FWD : Manage Forwarding. Type FWD Help for details.

EDITUSER (EU) : Manage Users. Type EU Help for details.

IMPORT : Import Messages from a file. Type IMPORT for details.

KH : Kills Held Messages.

K< Callsign : Kills message from [Callsign].

K> Callsign : Kills messages to [Callsign].

LH : List HELD messages.

LK : List KILLED messages

UH : Unhold messages. Either UH ALL or UH msg# msg#...